{"text_format":"1","workbook":"xlsx","n_sheets":28,"sheets":["トップページ","現況調査報告書","調査項目チェックリスト","結果表法19","結果表法43.44","結果表法20","結果表法22","結果表法23","結果表法35-2","結果表法28②","結果表法28③","結果表法31","結果表法32","結果表法36","結果表法37","結果表法28-2②","結果表法28-2③","結果表法28①","結果表法36床高","結果表法36階段","結果表法48","結果表法52","結果表法56","sheet2 (編集)","sheet3 (編集)","sheet1","sheet2","sheet3"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":23,"comments":21,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"トップページ","index":0,"n_rows":8,"n_cols":19,"rows_kept":8,"cut":false,"hidden":false,"merged":[]}
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"必要添付書類"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"□","現況調査報告書"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"□","調査項目チェックリスト"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"□","現況調査結果表"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"□","調査箇所を示した図面"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"□","直近の建築等の工事の検査済証の交付の事実又は工事の着手時がわかる書類"]

{"sheet":"現況調査報告書","index":1,"n_rows":64,"n_cols":36,"rows_kept":64,"cut":false,"hidden":false,"merged":[[45,0,49,3],[50,4,50,35],[51,4,51,35],[59,2,59,35],[60,2,60,35],[47,4,47,35],[48,4,48,35],[49,4,49,35],[61,1,61,35],[63,1,63,35],[53,4,53,35],[54,4,54,35],[55,4,55,35],[50,0,55,3],[57,2,57,35],[58,2,58,35],[52,4,52,35],[3,0,3,35],[5,1,5,34],[8,27,8,35],[7,2,7,21],[11,0,19,3],[12,4,12,9],[11,4,11,9],[19,10,19,35],[11,11,11,12],[11,14,11,16],[11,18,11,21],[11,24,11,30],[10,23,10,35],[13,4,13,9],[18,10,18,35],[14,11,14,12],[41,4,41,35],[42,4,42,35],[43,4,43,35],[44,4,44,35],[46,4,46,35],[37,10,37,35],[38,10,38,35],[37,5,38,9],[39,5,39,9],[40,5,40,9],[39,10,39,35],[40,10,40,18],[28,4,29,9],[28,20,29,25],[28,10,29,19],[28,29,28,34],[31,10,31,35],[33,10,33,35],[34,10,34,35],[35,10,35,35],[26,26,26,33],[26,34,26,35],[26,20,26,25],[12,10,12,35],[13,10,13,35],[22,10,22,35],[23,10,23,35],[24,10,24,35],[17,10,17,35],[20,0,27,3],[28,0,40,3],[14,14,14,18],[14,20,14,23],[14,25,14,28],[25,20,25,25],[25,10,25,19],[25,26,25,35],[27,20,27,25],[26,10,26,19],[27,10,27,17],[27,18,27,19],[36,10,36,35],[27,26,27,33],[27,34,27,35],[32,10,32,35],[41,0,44,3],[14,29,14,34],[31,5,31,9],[32,5,34,9],[35,5,36,9],[30,4,30,35],[18,4,19,9],[22,4,23,9],[17,4,17,9],[16,4,16,9],[14,4,15,9],[20,10,20,35],[20,4,20,9],[21,4,21,9],[15,10,15,35],[16,10,16,35]]}
[]
[]
[]
["現況調査報告書"]
[]
[null,"  ２．に記載の建築物の現況調査の結果を報告します。本報告書に記載の事項は、事実に相違ありません。"]
[]
[null,null,"所有者等の氏名"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"令和　　年　　月　　日"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"調査者氏名"]
["１．\n調査者\n（代表となる\n調査者）",null,null,null,"資格",null,null,null,null,null,"（","一級",null,"）","建築士",null,null,"（","広島県知事",null,null,null,"）","第",null,null,null,null,null,null,null,"号"]
[null,null,null,null,"氏名のフリガナ"]
[null,null,null,null,"氏名",null,null,null,null,null,{"$f":"IF(X11=\"\",\"\",X11)","v":""}]
[null,null,null,null,"勤務先",null,null,null,null,null,"（","一級",null,"）","建築士事務所",null,null,null,null,"（","広島県",null,null,null,"）","知事登録第",null,null,null,null,null,null,null,null,null,"号"]
[]
[null,null,null,null,"所在地"]
[null,null,null,null,"電話番号"]
[null,null,null,null,"その他調査者"]
[]
["２．\n調査対象建築物及び敷地の位置",null,null,null,"敷地の位置"]
[null,null,null,null,"防火地域",null,null,null,null,null,"□","防火地域",null,null,null,null,"□","準防火地域",null,null,null,null,null,"□","指定なし"]
[null,null,null,null,"その他の区域、地域、地区又は街区"]
[]
[null,null,null,null,"用途地域"]
[null,null,null,null,"現況用途",null,null,null,null,null,"一戸建ての住宅",null,null,null,null,null,null,null,null,null,"構造",null,null,null,null,null,"木造"]
[null,null,null,null,"階数",null,null,null,null,null,"地上　　階／地下　　階",null,null,null,null,null,null,null,null,null,"敷地面積",null,null,null,null,null,0,null,null,null,null,null,null,null,"㎡"]
[null,null,null,null,"建築面積",null,null,null,null,null,0,null,null,null,null,null,null,null,"㎡",null,"延べ面積",null,null,null,null,null,0,null,null,null,null,null,null,null,"㎡"]
["３．\n調査結果概要",null,null,null,"直近の建築等の工事の着手時点",null,null,null,null,null,"令和　　年　　月　　日",null,null,null,null,null,null,null,null,null,"検査済証の有無",null,null,null,null,null,"□","有","（","令和　　年　　月　　日",null,null,null,null,null,"）"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"□","無"]
[null,null,null,null,"現況調査結果※１"]
[null,null,null,null,null,"適合",null,null,null,null,"下記以外の規定"]
[null,null,null,null,null,"不適合\n（既存不適格）",null,null,null,null,"法第20条第1項（昭和56年6月1日）"]
[null,null,null,null,null,null,null,null,null,null,"法第28条の2（第3号に係る部分）（平成15年7月1日）"]
[null,null,null,null,null,null,null,null,null,null,"法第36条（階段の構造に係る部分）（平成12年6月1日） "]
[null,null,null,null,null,"不適合\n（その他）",null,null,null,null,"法第28条第1項 "]
[]
[null,null,null,null,null,"不明",null,null,null,null,"法第35条の2"]
[null,null,null,null,null,null,null,null,null,null,"法第37条 "]
[null,null,null,null,null,"その他特記事項",null,null,null,null,"平成12年バリアフリーに対応した段差解消及びトイレの更新工事"]
[null,null,null,null,null,"調査年月日",null,null,null,null,"令和　　年　　月　　日",null,null,null,null,null,null,null,null,"実施"]
["４．\n改変※２の有無及び概要",null,null,null,"1階居室の一部で窓がベニヤ板でふさがれている。"]
[]
[]
[]
["５．\n現況調査に用いた図書",null,null,null,"現況図面の作成 ",null,null,null,null,null,null,"□","有",null,"□","無"]
[null,null,null,null,"確認申請書の副本に添付された図面"]
[null,null,null,null,"壁量計算書（復元）"]
[null,null,null,null,"施工図面"]
[null,null,null,null,"専門調査会社に依頼した配筋調査結果報告書"]
["６．\n備考",null,null,null,"平成　　年に増築（　　　㎡）"]
[]
[]
[]
[]
[]
[null,"※１ 現況調査結果：次のとおり記載します。 "]
[null,null,"適合 ：現行の規定に適合している場合"]
[null,null,"不適合（既存不適格）：不適合である規定のうち、既存不適格である場合（既存不適格となった時点をかっこ書きで記載）"]
[null,null,"不適合（その他）：不適合である規定のうち、既存不適格ではない場合 "]
[null,null,"不明：やむを得ず調査ができず適合状況がわからない規定 "]
[null,"※２ 直近の建築等の工事に係る検査済証の交付を受けた後に、建築基準法令の規定に適合しない建築等に"]
[null,null,"該当しない行為（居室の採光上有効な窓をふさぐなど） "]
[null,"＊ 記入欄が不足する場合は、枠を拡大、行を追加して記入するか、別紙に必要な事項を記入し添えてください。 "]

{"sheet":"調査項目チェックリスト","index":2,"n_rows":164,"n_cols":5,"rows_kept":164,"cut":false,"hidden":false,"merged":[[58,4,59,4],[117,3,119,3],[162,2,163,2],[162,3,163,3],[159,1,160,1],[159,2,160,2],[148,1,158,1],[162,1,163,1],[149,4,152,4],[148,2,152,2],[153,4,154,4],[155,4,158,4],[153,2,158,2],[144,1,145,1],[144,2,145,2],[146,1,147,1],[146,2,147,2],[142,1,143,1],[142,2,143,2],[139,4,140,4],[139,2,141,2],[139,1,141,1],[135,1,136,1],[135,2,136,2],[137,1,138,1],[137,2,138,2],[120,4,122,4],[120,2,122,2],[120,1,122,1],[115,4,116,4],[114,2,116,2],[114,1,116,1],[129,2,130,2],[129,1,130,1],[133,1,134,1],[133,2,134,2],[123,1,127,1],[123,2,127,2],[123,4,127,4],[117,1,119,1],[109,1,113,1],[99,3,100,3],[99,2,100,2],[105,3,106,3],[101,2,107,2],[99,1,107,1],[117,4,119,4],[117,2,119,2],[90,4,93,4],[97,1,98,1],[97,2,98,2],[97,3,98,3],[97,4,98,4],[90,1,93,1],[90,2,93,2],[109,4,111,4],[112,3,113,3],[109,2,113,2],[69,4,70,4],[69,2,73,2],[69,1,70,1],[71,1,73,1],[55,4,57,4],[54,2,57,2],[54,1,57,1],[86,4,88,4],[83,2,88,2],[83,1,84,1],[85,1,88,1],[84,4,85,4],[79,1,82,1],[79,2,82,2],[81,4,82,4],[79,4,80,4],[79,3,80,3],[74,4,75,4],[74,2,78,2],[76,4,78,4],[74,1,75,1],[76,1,78,1],[60,1,61,1],[60,2,61,2],[51,4,52,4],[51,1,52,1],[39,2,40,2],[41,4,42,4],[41,2,42,2],[43,4,44,4],[45,3,46,3],[43,2,46,2],[27,2,28,2],[30,4,32,4],[30,2,33,2],[37,4,38,4],[34,4,35,4],[34,2,38,2],[13,4,14,4],[5,1,6,1],[5,2,6,2],[5,4,6,4],[8,1,9,1],[8,2,9,2],[8,4,9,4],[47,4,49,4],[47,2,49,2],[19,1,49,1],[19,2,23,2],[22,3,23,3],[20,3,21,3],[62,1,63,1],[62,2,63,2],[64,1,65,1],[64,2,65,2],[66,1,67,1],[66,2,67,2],[15,2,17,2],[15,1,17,1],[10,2,14,2],[10,1,14,1],[51,2,52,2],[58,1,59,1],[58,2,59,2]]}
[]
["■調査項目チェックリスト（調査対象の建築物に適用される規定と調査項目・調査方法）"]
["適用","規定","規定の内容","調査項目","調査方法"]
["敷地関係 （法第 43 条及び第 44 条は都市計画区域及び準都市計画区域内に限り適用）"]
["□","法19①","敷地の高さ","・道路との高低差","目視又は計測"]
["□","法19②","湿潤な土地等の衛生・安全対策","・敷地の湿潤状況、出水履歴、土地条件等","目視等及び土地条件図、治水地形分類図等を確認"]
[null,null,null,"・盛土、地盤改良等の有無"]
["□","法19③","敷地の排水","・敷地内の排水状況 ","目視等"]
["□","法19④","がけ崩れ対策 ","・がけの有無","目視等"]
[null,null,null,"・擁壁の設置状況"]
["□","法43①","接道","・都市計画区域・準都市計画区域の指定状況","市区町村の都市計画情報を確認"]
[null,null,null,"・特定行政庁による道路の指定状況 ","特定行政庁の指定道路図を確認"]
[null,null,null,"・特定行政庁による許可・認定の有無と適合状況","図書及び目視等"]
[null,null,null,"・道路との接道長さ","計測"]
[null,null,null,"・前面道路幅員"]
["□","法44①","道路内建築","・都市計画区域・準都市計画区域の指定状況","市区町村の都市計画情報を確認"]
[null,null,null,"・特定行政庁による道路の指定状況","特定行政庁の指定道路図を確認"]
[null,null,null,"・道路、建築物、擁壁等の位置","目視等"]
["構造関係"]
["□","法20①","基礎","・立ち上がり部分の構造、材料及び寸法","目視等及び計測"]
[null,null,null,"・配筋の状況","・電磁誘導法　　又は"]
[null,null,null,null,"・電磁波レーダー法による鉄筋探査及びはつり出し"]
[null,null,null,"・（令第38条第4項の構造計算による場合）\n　コンクリートの強度","・コンクリート圧縮試験　　又は"]
[null,null,null,null,"・シュミットハンマー試験"]
[null,null,"屋根ふき材外装材等 ","・緊結等の状況","目視等"]
[null,null,"木材","・構造耐力上主要な部分に使用されている木材の状況","目視等"]
[null,null,"土台及び基礎","・土台の緊結等の状況 ","目視等"]
[null,null,"柱の小径","・欠込み等の有無","目視等"]
[null,null,null,"・部材寸法（柱の小径）","計測"]
[null,null,"はり等の横架材","・欠込み等の有無","目視等"]
[null,null,"筋かい","・柱梁接合部及び筋かいの金物の有無及び","目視等"]
[null,null,null,"　金物種類、緊結の状況"]
[null,null,null,"・欠込み等の有無"]
[null,null,null,"・筋かいの部材寸法","計測"]
[null,null,"軸組等","・筋かい、耐力壁の位置","目視等"]
[null,null,null,"・金物種類"]
[null,null,null,"・筋かい、耐力壁の部材寸法等の状況","目視等及び計測"]
[null,null,null,"・壁量計算による必要壁量及び存在壁量、配置の確認","壁量計算"]
[null,null,null,"・壁配置のバランス"]
[null,null,"継手又は仕口","・柱梁接合部の金物の有無及び金物種類、緊結の状況","目視等"]
[null,null,null,"・筋かいの部材寸法 ","計測"]
[null,null,"防腐措置","・腐りやすい構造である部分の下地材","目視等"]
[null,null,null,"・柱、筋かい、土台の防腐・防蟻処理の状況"]
[null,null,"塀","・高さ、厚さ","目視等及び計測"]
[null,null,null,"・控え壁、基礎の有無"]
[null,null,null,"・配筋の状況","・電磁誘導法　　又は"]
[null,null,null,null,"・電磁波レーダー法による鉄筋探査及びはつり出し"]
[null,null,"建築設備の構造強度","・給湯設備の満水時の質量","・目視等　　及び\n・設備の型番から仕様を確認"]
[null,null,null,"・給湯設備の形状"]
[null,null,null,"・給湯設備の緊結状況"]
["適用","規定","規定の内容","調査項目","調査方法"]
["□","法20②","基準の適用上別の建築物みなす部分","・相互に応力を伝えない構造方法のみで","目視等"]
[null,null,null,"　接する建築物の部分の有無"]
["防火関係"]
["□","法61①","防火地域・準防火地域内の建築物","・防火地域、準防火地域の指定状況 ","市区町村の都市計画情報を確認"]
[null,null,null,"・建築物の規模に応じた耐火建築物、準耐火","・目視等　　又は\n・設備の認定シール等を確認"]
[null,null,null,"　建築物等の種別及び構造材の状況"]
[null,null,null,"・延焼のおそれのある部分の防火設備の位置、形状等"]
["□","法61②","基準の適用上別の建築物みなす部分 ","・火熱遮断壁等により分離されている建築物","・目視等"]
[null,null,null,"　の部分の有無 "]
["□","法62","屋根","・防火地域、準防火地域の指定状況 ","市区町村の都市計画情報を確認"]
[null,null,null,"・屋根材の状況 ","目視等"]
["□","法22①","屋根","・法第 22 条区域の指定状況","特定行政庁による指定状況を確認"]
[null,null,null,"・屋根ふき材の状況","目視等"]
["□","法23 ","外壁","・法第 22 条区域の指定状況","特定行政庁による指定状況を確認"]
[null,null,null,"・外壁材の状況 ","目視等"]
["□","法35の2 ","内装 ","・火気使用室の有無","・目視等　　又は"]
[null,null,null,"・内装材","・材料の認定シール等を確認"]
["設備関係"]
["□","法28②\n法36","換気設備\n（調理室等を除く）","・開口部の面積、位置","目視等及び計測"]
[null,null,null,"・給気口、排気口の位置"]
[null,"（給水、排水その他の配管設備の設置及び構造に係る部分）",null,"・機械換気設備の性能等","・風量測定　　又は"]
[null,null,null,"・換気設備の有効換気量","・設備の型番から性能等を確認"]
[null,null,null,"・居室の床面積 ","計測"]
["□","法28③\n法36","換気設備\n（調理室等）","・ガス設備等の有無","目視等"]
[null,null,null,"・給気口、排気口の位置"]
[null,"（給水、排水その他の配管設備の設置及び構造に係る部分）",null,"・火気設備の出力等","・風量測定　　又は\n・設備の型番から性能等を確認"]
[null,null,null,"・機械換気設備の性能等"]
[null,null,null,"・換気設備の有効換気量"]
["□","法31①\n法 36\n（便所の設置及び構造に係る部分）","便所\n（処理区域内）","・公共下水道の処理区域","処理区域の公示を確認"]
[]
[null,null,null,"・採光及び換気のための窓又はそれに代わる","目視等"]
[null,null,null,"　照明、換気設備の有無"]
["□","法31②\n法36","便所\n（処理区域外）","・公共下水道の処理区域","処理区域の公示を確認"]
[null,null,null,"・浄化槽の処理性能　又は","浄化槽の保守点検結果及び設備の型番から性能等を確認"]
[null,"（便所の設置及び構造並びに浄化槽の構造に係る部分）",null,"・くみ取便所の構造"]
[null,null,null,"・採光及び換気のための窓又はそれに代わる","目視等"]
[null,null,null,"　照明、換気設備の有無"]
[null,null,null,"・漏水の有無"]
["□","法32","電気設備 ","・不具合の有無","目視等"]
["□","法36\n（給水、排水その他の配管設備の設置及び構造に係る部分）","給排水設備",null,"目視等"]
[null,null,null,"・配管設備の設置状況"]
[null,null,null,"・漏水等不具合の有無 "]
[]
["適用","規定","規定の内容","調査項目","調査方法"]
["材料関係"]
["□","法37","建築材料","・基礎のコンクリート、鉄筋の JIS への適合状況","図書等により使用材料の仕様を確認"]
["□","法28の2\n二","石綿 ","・石綿の吹付けの有無","目視等"]
[]
["□","法28の2\n三","クロルピリホス","・添加の有無（添加されている場合は、\n　5年以上が経過していること）","・図書等により仕様を確認 　又は"]
[null,null,null,null,"・目視等"]
["□",null,"ホルムアルデヒド","・使用の有無（使用されている場合は、"]
[null,null,null,"　5年以上が経過していること）","・図書等による仕様を確認　　又は"]
[null,null,null,"・換気経路（建具のアンダーカット、ガラリ等の有無）","・目視等"]
[null,null,null,"・給気口、排気口の位置"]
[null,null,null,"・換気設備の有効換気量","・風量測定　　又は"]
[null,null,null,null,"・設備の型番から性能等を確認"]
[null,null,null,"・居室の面積、天井高さ","計測"]
["一般構造関係"]
["□","法28①\n法36\n（居室の採光面積に係る部分）","採光","・居室の面積","計測"]
[null,null,null,"・開口部の寸法、開口中心からの垂直距離"]
[null,null,null,"・外壁と隣地境界線等との距離"]
[null,null,null,"・照明設備の性能等","・床面における照度測定　　又は"]
[null,null,null,null,"・設備の型番から各種性能を確認"]
["□","法29","地階における居室","・居室の面積 ","計測"]
[null,null,null,"・からぼり等の有無","目視等"]
[null,null,null,"・地面に接する外壁等の構造"]
["□","法36\n（天井及び床の高さに係る部分）","居室の天井及び床の高さ","・居室の天井高さ\n・最下階の居室の床の高さ ","計測"]
[]
[]
["□","法36\n（床の防湿方法に係る部分）","居室の床の防湿方法","・最下階の床の材料","目視等"]
[null,null,null,"・床下の防湿措置の状況"]
[null,null,null,"・外壁の床下換気孔の状況 "]
["□","法36\n（階段の構造に係る部分）","階段","・階段及び踊場の幅員","目視等及び計測"]
[null,null,null,"・階段の蹴上げ、踏面の寸法"]
[null,null,null,"・手すりの設置状況、出幅の寸法"]
[null,null,null,"・踊場の設置状況"]
[null,null,null,"・階段に代わる傾斜路の設置状況"]
["用途関係 （都市計画区域及び準都市計画区域内に限り適用）"]
["□","法48\n①～⑭","用途","・用途地域の指定状況","市区町村の都市計画情報を確認"]
[null,null,null,"・兼用用途の有無及び当該用途に供する床面積","目視等及び計測"]
["適用","規定","規定の内容","調査項目","調査方法"]
["形態関係 （都市計画区域及び準都市計画区域内に限り適用）"]
["□","法47","壁面線","・壁面線の指定状況 ","特定行政庁による指定状況を確認"]
[null,null,null,"・壁面線と外壁との距離","計測"]
["□","法52\n①,⑦","用途地域等に基づく容積率","・指定容積率","市区町村の都市計画情報を確認"]
[null,null,null,"・建築物の延べ面積及び敷地面積","計測"]
["□","法52\n②,⑦","前面道路の幅員に\n基づく容積率","・用途地域等の指定状況","市区町村の都市計画情報を確認"]
[null,null,null,"・前面道路の幅員","計測"]
["□","法53\n①,②","建蔽率","・指定建蔽率","市区町村の都市計画情報を確認"]
[null,null,null,"・防火地域、準防火地域の指定状況"]
[null,null,null,"・建築物の建築面積及び敷地面積","計測"]
["□","法53の2\n①","最低敷地面積","・敷地面積の最低限度の指定状況","市区町村の都市計画情報を確認"]
[null,null,null,"・敷地面積","計測"]
["□","法54①","外壁後退距離","・外壁の後退距離の限度の指定状況 ","市区町村の都市計画情報を確認"]
[null,null,null,"・外壁から敷地境界線までの距離 ","計測"]
["□","法55①","絶対高さ制限","・高さの限度の指定状況","市区町村の都市計画情報を確認"]
[null,null,null,"・建築物の高さ ","計測"]
["□","法56①","道路高さ制限","・用途地域の指定状況","市区町村の都市計画情報を確認"]
[null,null,null,"・前面道路幅員","計測"]
[null,null,null,"・前面道路との高低差"]
[null,null,null,"・建築物の高さ"]
[null,null,null,"・道路境界線との距離"]
[null,null,"北側高さ制限","・用途地域の指定状況","市区町村の都市計画情報及び条例の制定状況を確認"]
[null,null,null,"・日影による高さ制限の対象区域の指定状況"]
[null,null,null,"・真北の方角","計測"]
[null,null,null,"・真北方向の境界線との距離"]
[null,null,null,"・北側隣地との高低差"]
[null,null,null,"・建築物の高さ"]
["□","法58①","高度地区内の建築物","・高度地区の指定状況","市区町村の都市計画情報を確認"]
[null,null,null,"・建築物の高さ ","計測"]
["その他（条例により付加された制限）"]
["□","法39,40,\n68の2他","地方公共団体の条例による制限","・地方公共団体の条例による制限の有無及び内容","・条例の制定状況を確認"]
[null,null,null,null,"・制限の内容に応じて確認方法を検討"]

{"sheet":"結果表法19","index":3,"n_rows":29,"n_cols":19,"rows_kept":29,"cut":false,"hidden":false,"merged":[[3,0,3,3],[4,0,7,3],[8,0,27,3],[28,0,47,3],[2,18,2,31],[4,18,7,31],[2,0,2,3],[2,4,2,17],[3,4,3,17],[3,18,3,31],[4,4,7,17]]}
[]
["■現況調査結果表"]
["規定",null,null,null,"法第19条第1項",null,null,null,null,null,null,null,null,null,null,null,null,null,"法第19条第3項"]
["適合状況",null,null,null,"適合",null,null,null,null,null,null,null,null,null,null,null,null,null,"適合"]
["調査結果",null,null,null,"敷地は前面道路の境よりも高い位置にある。",null,null,null,null,null,null,null,null,null,null,null,null,null,"宅内の雨水処理のための浸透ます及び汚水放流先の公共下水について宅内の引き込み有り。"]
[]
[]
[]
["調査箇所の写真"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["詳細図等"]

{"sheet":"結果表法43.44","index":4,"n_rows":29,"n_cols":19,"rows_kept":29,"cut":false,"hidden":false,"merged":[[28,0,47,3],[2,0,2,3],[2,4,2,17],[2,18,2,31],[3,0,3,3],[3,4,3,17],[3,18,3,31],[4,0,7,3],[4,4,7,17],[4,18,7,31],[8,0,27,3]]}
[]
["■現況調査結果表"]
["規定",null,null,null,"法第43条第1項",null,null,null,null,null,null,null,null,null,null,null,null,null,"法第44条第1項"]
["適合状況",null,null,null,"適合",null,null,null,null,null,null,null,null,null,null,null,null,null,"適合"]
["調査結果",null,null,null,"敷地は幅員6ｍの市道に2ｍ以上接している。",null,null,null,null,null,null,null,null,null,null,null,null,null,"道路内及び道路に突き出して建築されているものはない。"]
[]
[]
[]
["調査箇所の写真"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["詳細図等"]

{"sheet":"結果表法20","index":5,"n_rows":76,"n_cols":6,"rows_kept":76,"cut":false,"hidden":false,"merged":[[2,0,2,3],[3,0,3,3],[2,4,2,31],[3,4,3,31],[55,0,74,3],[46,4,46,31],[47,5,51,31],[52,4,52,31],[53,5,54,31],[75,0,94,3],[4,4,4,31],[4,0,54,3],[23,5,27,31],[28,4,28,31],[29,5,33,31],[34,4,34,31],[35,5,39,31],[40,4,40,31],[5,5,9,31],[10,4,10,31],[11,5,15,31],[16,4,16,31],[17,5,21,31],[22,4,22,31],[41,5,45,31]]}
[]
["■現況調査結果表"]
["規定",null,null,null,"法第20条第１項"]
["適合状況",null,null,null,"不適合（既存不適格）"]
["調査結果",null,null,null,"①基礎"]
[null,null,null,null,null,"建物北西側基礎１箇所において、目視、計測により基礎の構造及び材料、寸法を確認した結果、確認申請書の副本の図面どおりに施工されていた。\n同箇所において、基礎の立上り部分の配筋の状況について、専門の調査会社に調査（別添）を依頼した結果によれば、せん断補強筋の配筋間隔が約500mmと広く、現行の基準は満たしていない。\n異なる構造の基礎は併用されていないため、直近の建築時の基準には適合する。"]
[]
[]
[]
[]
[null,null,null,null,"②土台"]
[null,null,null,null,null,"土台に使用されている木材について目視による調査をしたところ、適切に施工されており、割れや欠け等の耐力上の欠点はみられなかった。\nスイッチプレートからファイバースコープを用いて内部を確認したところ、アンカーボルトにより土台が基礎に緊結されていることを確認した。"]
[]
[]
[]
[]
[null,null,null,null,"③柱"]
[null,null,null,null,null,"押入れの天井にある点検口から柱を確認し、寸法を実測した結果を確認申請書の副本に添付された図面と照合し、問題ないことを確認した。\n欠込み等はなく、柱に使用された木材の品質に耐力上の欠点はみられなかった。"]
[]
[]
[]
[]
[null,null,null,null,"④はり"]
[null,null,null,null,null,"押入れの天井にある点検口からはりを確認し、耐力上支障がある欠込みはなく、はりに使用された木材の品質に耐力上の欠点はみられなかった。"]
[]
[]
[]
[]
[null,null,null,null,"⑤筋かい"]
[null,null,null,null,null,"確認申請書の副本の図面に基づき、壁量計算を行った結果、現行基準には適合しないものの、建築当時の基準に適合していることを確認した。\nまた、図面と現地の整合を、押入れの天井にある点検口から目視で確認するとともに、各階1箇所、壁の一部を破壊し内部を確認したところ、当該部分は計画どおり筋かいが設置されていたことから、図面どおり施工されているものと判断した。\nさらに、筋かいの端部はくぎで緊結されていることを確認した。\nなお、筋かいに使用された木材の品質に耐力上の欠点や欠き込みはみられなかった。"]
[]
[]
[]
[]
[null,null,null,null,"⑥接合部（継手・仕口）"]
[null,null,null,null,null,"押入れの天井にある点検口から目視により、継手・仕口を確認したところ、ボルト締、かすがい打又は込み栓打により緊結されており、現行の基準には適合しないものの、直近の建築時の規定に適合していることを確認した。"]
[]
[]
[]
[]
[null,null,null,null,"⑦屋根ふき材"]
[null,null,null,null,null,"2階廊下から1階下屋部分の屋根を目視により確認したところ、瓦屋根が下地に銅線で緊結されていたが、釘等による緊結はされていない。"]
[]
[]
[]
[]
[null,null,null,null,"⑧塀"]
[null,null,null,null,null,"実測の結果、高さ1.2m、厚み15cmであり、控え壁の設置は不要。目視により調査した結果、塀にひび割れはなく、倒壊の危険性はないと判断した。\n専門の調査会社に調査（別添）を依頼した結果から、塀内部の配筋間隔、鉄筋径は現行の基準を満たしていると判断した。"]
[]
[]
[]
[]
[null,null,null,null,"⑨給湯設備"]
[null,null,null,null,null,"給湯機（品番：○○○○）上部が壁に固定され、転倒防止措置が講じ\nられていた。"]
[]
["調査箇所の写真"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["詳細図等"]

{"sheet":"結果表法22","index":6,"n_rows":29,"n_cols":5,"rows_kept":29,"cut":false,"hidden":false,"merged":[[8,0,27,3],[28,0,47,3],[4,4,7,31],[2,0,2,3],[3,0,3,3],[2,4,2,31],[3,4,3,31],[4,0,7,3]]}
[]
["■現況調査結果表"]
["規定",null,null,null,"法第22条第1項"]
["適合状況",null,null,null,"適合"]
["調査結果",null,null,null,"法第22条区域に指定されている。\n\n2階から1階屋根の使用材料を目視により確認したところ、粘土瓦であることを確認した。"]
[]
[]
[]
["調査箇所の写真"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["詳細図等"]

{"sheet":"結果表法23","index":7,"n_rows":29,"n_cols":5,"rows_kept":29,"cut":false,"hidden":false,"merged":[[8,0,27,3],[28,0,47,3],[2,0,2,3],[2,4,2,31],[3,0,3,3],[3,4,3,31],[4,0,7,3],[4,4,7,31]]}
[]
["■現況調査結果表"]
["規定",null,null,null,"法第23条"]
["適合状況",null,null,null,"適合"]
["調査結果",null,null,null,"法第22条区域に指定されている。\n\n北西側1階の外壁材を目視により確認したところ、窯業系サイディングであることを確認した。竣工図面に記載されている品番より商品を特定し、大臣認定が取得されていることを確認した。"]
[]
[]
[]
["調査箇所の写真"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["詳細図等"]

{"sheet":"結果表法35-2","index":8,"n_rows":29,"n_cols":5,"rows_kept":29,"cut":false,"hidden":false,"merged":[[8,0,27,3],[28,0,47,3],[2,0,2,3],[2,4,2,31],[3,0,3,3],[3,4,3,31],[4,0,7,3],[4,4,7,31]]}
[]
["■現況調査結果表"]
["規定",null,null,null,"法第35条の2"]
["適合状況",null,null,null,"不明"]
["調査結果",null,null,null,"火気使用室である台所に使用されている内装材の仕様が現地では判別できなかった。"]
[]
[]
[]
["調査箇所の写真"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["詳細図等"]

{"sheet":"結果表法28②","index":9,"n_rows":30,"n_cols":5,"rows_kept":30,"cut":false,"hidden":false,"merged":[[9,0,28,3],[29,0,48,3],[2,0,3,3],[2,4,2,31],[3,4,3,31],[4,0,4,3],[4,4,4,31],[5,0,8,3],[5,4,8,31]]}
[]
["■現況調査結果表"]
["規定",null,null,null,"法第28条第2項"]
[null,null,null,null,"法第36条（給水、排水その他の配管設備の設置及び構造に係る部分）"]
["適合状況",null,null,null,"適合"]
["調査結果",null,null,null,"自然換気が設けられ、有効換気計算表のとおり、居室の開口部の有効換気面積は各必要換気面積を満たしている。\nまた、給気口は天井の高さの1/2以下の高さに設置され、排気口も適切な位置に設置されている。"]
[]
[]
[]
["調査箇所の写真"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["詳細図等"]

{"sheet":"結果表法28③","index":10,"n_rows":30,"n_cols":5,"rows_kept":30,"cut":false,"hidden":false,"merged":[[9,0,28,3],[29,0,48,3],[3,4,3,31],[2,0,3,3],[2,4,2,31],[4,0,4,3],[4,4,4,31],[5,0,8,3],[5,4,8,31]]}
[]
["■現況調査結果表"]
["規定",null,null,null,"法第28条第3項"]
[null,null,null,null,"法第36条（給水、排水その他の配管設備の設置及び構造に係る部分）"]
["適合状況",null,null,null,"適合"]
["調査結果",null,null,null,"火気使用室（1階台所）の有効換気量は、設置されている換気扇付近で風量計測をすると400㎥／h、必要換気量は30×0.93（㎥）×10.78（kW=300.76㎥／h であるため、有効換気量＞必要換気量を満たしている。\nまた、火気使用室における換気扇の設置高さは、天井から 80cm 以内の位置にある。"]
[]
[]
[]
["調査箇所の写真"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["詳細図等"]

{"sheet":"結果表法31","index":11,"n_rows":30,"n_cols":5,"rows_kept":30,"cut":false,"hidden":false,"merged":[[9,0,28,3],[29,0,48,3],[2,0,3,3],[2,4,2,31],[3,4,3,31],[4,0,4,3],[4,4,4,31],[5,0,8,3],[5,4,8,31]]}
[]
["■現況調査結果表"]
["規定",null,null,null,"法第31条"]
[null,null,null,null,"法第36条（便所の設置及び構造に係る部分）"]
["適合状況",null,null,null,"適合"]
["調査結果",null,null,null,"公共下水道の処理区域内であり、公共下水道に接続された水洗便所が設置されている。また、便所内には窓及び換気扇が設置されている。"]
[]
[]
[]
["調査箇所の写真"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["詳細図等"]

{"sheet":"結果表法32","index":12,"n_rows":29,"n_cols":5,"rows_kept":29,"cut":false,"hidden":false,"merged":[[8,0,27,3],[28,0,47,3],[2,0,2,3],[2,4,2,31],[3,0,3,3],[3,4,3,31],[4,0,7,3],[4,4,7,31]]}
[]
["■現況調査結果表"]
["規定",null,null,null,"法第32条"]
["適合状況",null,null,null,"適合"]
["調査結果",null,null,null,"分電盤を確認し、通電状況には問題なかった。"]
[]
[]
[]
["調査箇所の写真"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["詳細図等"]

{"sheet":"結果表法36","index":13,"n_rows":29,"n_cols":5,"rows_kept":29,"cut":false,"hidden":false,"merged":[[8,0,27,3],[28,0,47,3],[2,0,2,3],[2,4,2,31],[3,0,3,3],[3,4,3,31],[4,0,7,3],[4,4,7,31]]}
[]
["■現況調査結果表"]
["規定",null,null,null,"法第36条（給水、排水その他の配管設備の設置及び構造に係る部分） "]
["適合状況",null,null,null,"適合"]
["調査結果",null,null,null,"飲料水の配管設備とその他の配管設備は直接連結されていないことを確認した。飲料水の逆流防止のための措置が講じられていることを確認した。\n\n給水タンクは衛生上支障がない構造であることを確認した。\n\n排水のための配管設備は、排水トラップが設置されていることを確認した。排水設備の末端は公共下水道に接続されていることを確認した。"]
[]
[]
[]
["調査箇所の写真"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["詳細図等"]

{"sheet":"結果表法37","index":14,"n_rows":29,"n_cols":5,"rows_kept":29,"cut":false,"hidden":false,"merged":[[8,0,27,3],[28,0,47,3],[2,0,2,3],[2,4,2,31],[3,0,3,3],[3,4,3,31],[4,0,7,3],[4,4,7,31]]}
[]
["■現況調査結果表"]
["規定",null,null,null,"法第37条 "]
["適合状況",null,null,null,"不明"]
["調査結果",null,null,null,"基礎のコンクリート及び鉄筋の品質については、図書が残っておらず確認できなかった。 "]
[]
[]
[]
["調査箇所の写真"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["詳細図等"]

{"sheet":"結果表法28-2②","index":15,"n_rows":29,"n_cols":5,"rows_kept":29,"cut":false,"hidden":false,"merged":[[8,0,27,3],[28,0,47,3],[2,0,2,3],[2,4,2,31],[3,0,3,3],[3,4,3,31],[4,0,7,3],[4,4,7,31]]}
[]
["■現況調査結果表"]
["規定",null,null,null,"法第28条の2（第二号に係る部分）"]
["適合状況",null,null,null,"適合"]
["調査結果",null,null,null,"押入れの天井にある点検口から小屋裏内部を目視した結果、吹付による仕上げや断熱材の使用はなかった。"]
[]
[]
[]
["調査箇所の写真"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["詳細図等"]

{"sheet":"結果表法28-2③","index":16,"n_rows":29,"n_cols":5,"rows_kept":29,"cut":false,"hidden":false,"merged":[[8,0,27,3],[28,0,47,3],[2,0,2,3],[2,4,2,31],[3,0,3,3],[3,4,3,31],[4,0,7,3],[4,4,7,31]]}
[]
["■現況調査結果表"]
["規定",null,null,null,"法第28条の2（第三号に係る部分） "]
["適合状況",null,null,null,"不適合（既存不適格）"]
["調査結果",null,null,null,"クロルピリホスの添加の有無は不明だが、竣工後5年以上経過していることから、制限の対象となる建築材料に該当しない。 \n\n内装材にホルムアルデヒドが使用されているが、５年以上経過していることから、制限の対象となる建築材料に該当しない。 \n\n令第20条の8８第1号に規定された機械換気設備は設置されていない"]
[]
[]
[]
["調査箇所の写真"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["詳細図等"]

{"sheet":"結果表法28①","index":17,"n_rows":30,"n_cols":5,"rows_kept":30,"cut":false,"hidden":false,"merged":[[9,0,28,3],[29,0,48,3],[2,0,3,3],[3,4,3,31],[2,4,2,31],[4,0,4,3],[4,4,4,31],[5,0,8,3],[5,4,8,31]]}
[]
["■現況調査結果表"]
["規定",null,null,null,"法第28条第1項"]
[null,null,null,null,"法第36条（居室の採光面積に係る部分） "]
["適合状況",null,null,null,"不適合（その他）"]
["調査結果",null,null,null,"採光適合確認表のとおり、洋室1以外の居室については、有効採光面積が必要採光面積以上となっている。\n\n洋室1の窓がベニヤ板でふさがれており、採光上有効な面積を確保できていない。 "]
[]
[]
[]
["調査箇所の写真"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["詳細図等"]

{"sheet":"結果表法36床高","index":18,"n_rows":29,"n_cols":19,"rows_kept":29,"cut":false,"hidden":false,"merged":[[28,0,47,3],[2,0,2,3],[2,4,2,17],[2,18,2,31],[3,0,3,3],[3,4,3,17],[3,18,3,31],[4,0,7,3],[4,4,7,17],[4,18,7,31],[8,0,27,3]]}
[]
["■現況調査結果表"]
["規定",null,null,null,"法第36条（天井及び床の高さに係る部分）",null,null,null,null,null,null,null,null,null,null,null,null,null,"法第36条（床の防湿方法に係る部分） "]
["適合状況",null,null,null,"適合",null,null,null,null,null,null,null,null,null,null,null,null,null,"適合"]
["調査結果",null,null,null,"居室の天井高さは、現地で実測した結果2.4ｍ≧2.1ｍであり、要高さを満たしている。",null,null,null,null,null,null,null,null,null,null,null,null,null,"床の高さは、現地で実測した結果、直下の地面からその床の上面まで69cm≧45cmであり、適切に換気孔が設けられている。"]
[]
[]
[]
["調査箇所の写真"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["詳細図等"]

{"sheet":"結果表法36階段","index":19,"n_rows":29,"n_cols":5,"rows_kept":29,"cut":false,"hidden":false,"merged":[[8,0,27,3],[28,0,47,3],[2,0,2,3],[2,4,2,31],[3,0,3,3],[3,4,3,31],[4,0,7,3],[4,4,7,31]]}
[]
["■現況調査結果表"]
["規定",null,null,null,"法第36条（階段の構造に係る部分） "]
["適合状況",null,null,null,"不適合（既存不適格）"]
["調査結果",null,null,null,"階段の各部寸法は下表のとおり、現行の規定に適合している。 手すりは設置されていない。"]
[]
[]
[]
["調査箇所の写真"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["詳細図等"]

{"sheet":"結果表法48","index":20,"n_rows":29,"n_cols":5,"rows_kept":29,"cut":false,"hidden":false,"merged":[[8,0,27,3],[28,0,47,3],[2,0,2,3],[2,4,2,31],[3,0,3,3],[3,4,3,31],[4,0,7,3],[4,4,7,31]]}
[]
["■現況調査結果表"]
["規定",null,null,null,"法第48条第4項 "]
["適合状況",null,null,null,"適合"]
["調査結果",null,null,null,"用途地域は第二種中高層住居専用地域であり、建築物の用途は一戸建ての専用住宅であるため、適合している。"]
[]
[]
[]
["調査箇所の写真"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["詳細図等"]

{"sheet":"結果表法52","index":21,"n_rows":35,"n_cols":23,"rows_kept":35,"cut":false,"hidden":false,"merged":[[2,22,2,30],[3,22,3,30],[4,22,13,30],[4,0,13,3],[14,0,33,3],[34,0,53,3],[4,4,13,12],[4,13,13,21],[2,0,2,3],[3,0,3,3],[2,4,2,12],[3,4,3,12],[2,13,2,21],[3,13,3,21]]}
[]
["■現況調査結果表"]
["規定",null,null,null,"法第52条第1項 ",null,null,null,null,null,null,null,null,"法第52条第2項 ",null,null,null,null,null,null,null,null,"法第53条第1項 "]
["適合状況",null,null,null,"適合",null,null,null,null,null,null,null,null,"適合",null,null,null,null,null,null,null,null,"適合"]
["調査結果",null,null,null,"敷地面積、延べ床面積について実測した値は確認申請書の副本に添付された図面と照合し整合を確認した。敷地内には、当該図面に記載された建築物以外の建築物はなかった。\n\n指定容積率は150%であり、延べ床面積は面積表のとおり適合している。",null,null,null,null,null,null,null,null,"敷地面積、床面積は左記のとおり。 前面道路の幅員は６ｍであり、幅員に乗じる数値は4/10であるため、240％となる。 延べ床面積は面積表のとおり適合している。",null,null,null,null,null,null,null,null,"敷地面積、建築面積について実測した値は確認申請書の副本に添付された図面と照合し整合を確認した。敷地内には、当該図面に記載された建築物以外の建築物はなかった。 指定建蔽率は50%であり、建築面積は面積表のとおり適合している。"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["調査箇所の写真"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["詳細図等"]

{"sheet":"結果表法56","index":22,"n_rows":29,"n_cols":19,"rows_kept":29,"cut":false,"hidden":false,"merged":[[28,0,47,3],[2,0,2,3],[2,4,2,17],[2,18,2,31],[3,0,3,3],[3,4,3,17],[3,18,3,31],[4,0,7,3],[4,4,7,17],[4,18,7,31],[8,0,27,3]]}
[]
["■現況調査結果表"]
["規定",null,null,null,"法第56条第1項 ",null,null,null,null,null,null,null,null,null,null,null,null,null,"法第58条第1項 "]
["適合状況",null,null,null,"適合",null,null,null,null,null,null,null,null,null,null,null,null,null,"適合"]
["調査結果",null,null,null,"建築物の高さを実測した値を確認申請書の副本に添付された図面と照合し、整合を確認した。\n\n調査時点における用途地域に応じた斜線勾配は詳細図に示すとおりで、高さは適合している。",null,null,null,null,null,null,null,null,null,null,null,null,null,"建築物の高さを実測した値を確認申請書の副本に添付された図面と照合し、整合を確認した。\n\n調査時点における高度地区の内容は詳細図に示すとおりで、高さは適合している。"]
[]
[]
[]
["調査箇所の写真"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["詳細図等"]

{"sheet":"sheet2 (編集)","index":23,"n_rows":43,"n_cols":9,"rows_kept":43,"cut":false,"hidden":true,"merged":[[33,8,33,9],[31,5,31,7],[33,5,33,7],[39,8,39,9],[40,8,40,9],[41,8,41,9],[40,1,41,1],[39,2,41,2],[40,3,41,4],[41,5,41,7],[35,8,35,9],[36,8,36,9],[37,1,38,1],[37,2,38,2],[37,3,38,4],[37,5,37,7],[37,8,37,9],[38,8,38,9],[38,5,38,7],[39,3,39,4],[39,5,39,7],[40,5,40,7],[34,1,34,2],[36,5,36,7],[2,2,3,2],[24,8,24,9],[25,8,25,9],[32,5,32,7],[30,8,30,9],[29,8,29,9],[28,8,28,9],[31,8,31,9],[32,8,32,9],[24,3,24,4],[24,5,24,7],[25,3,25,4],[25,5,25,7],[26,3,26,4],[26,5,26,7],[22,3,22,4],[23,3,23,4],[22,5,23,7],[18,3,18,4],[18,5,18,7],[15,8,17,9],[14,1,14,2],[15,3,15,4],[15,5,15,7],[5,1,6,1],[5,2,6,2],[5,3,6,4],[5,8,5,9],[12,5,12,7],[12,8,12,9],[4,1,4,2],[6,5,6,7],[6,8,6,9],[7,5,7,7],[7,8,7,9],[7,1,8,1],[7,2,8,2],[7,3,8,4],[9,1,10,1],[9,2,10,2],[9,3,10,4],[9,5,9,7],[9,8,9,9],[10,5,10,7],[10,8,10,9],[11,1,12,1],[11,2,12,2],[11,3,12,4],[35,1,36,1],[35,2,36,2],[35,3,36,4],[35,5,35,7],[27,1,27,2],[28,3,28,4],[28,5,28,7],[29,3,29,4],[29,5,29,7],[30,2,33,2],[30,3,30,4],[30,5,30,7],[31,1,33,1],[31,3,33,4],[16,3,16,4],[16,5,16,7],[22,8,23,9],[19,3,19,4],[19,5,19,7],[20,3,20,4],[20,5,20,7],[21,3,21,4],[21,5,21,7],[21,8,21,9],[20,8,20,9],[18,8,19,9],[17,3,17,4],[17,5,17,7],[13,3,13,4],[13,5,13,7],[13,8,13,9],[8,5,8,7],[8,8,8,9],[1,5,1,7],[1,8,1,9],[11,5,11,7],[11,8,11,9],[2,3,2,4],[2,5,2,7],[2,8,2,9],[3,3,3,4],[3,5,3,7],[3,8,3,9],[1,3,1,4]]}
[]
[null,"適用","法令","規定の内容",null,"調査項目",null,null,"調査方法"]
[null,null,null,null,null,null,null,null,"・電磁波レーダー法による鉄筋探査及び\n　はつり出し"]
[null,"□",null,"建築設備の構造\n強度",null,"・給湯設備の満水時の質量\n・給湯設備の形状\n・給湯設備の緊結状況",null,null,"・設備の型番から仕様を確認\n・目視等"]
[null,"防火関係"]
[null,"□","法61","防火地域・準防火地域内の建築物",null,"・防火地域、準防火地域の指定状況",null,null,"市区町村の都市計画情報を確認"]
[null,null,null,null,null,"・建築物の規模に応じた耐火建築物、準耐火建築物等の種別及び構造材の状況\n・延焼のおそれのある部分の防火設備の位置、形状等",null,null,"・目視等　又は\n・設備の認定シール等を確認"]
[null,"□","法62","屋根",null,"・防火地域、準防火地域の指定状況",null,null,"市区町村の都市計画情報を確認"]
[null,null,null,null,null,"・屋根材の状況",null,null,"目視等"]
[null,"□","法22","屋根",null,"・法第22条区域の指定状況",null,null,"特定行政庁による指定状況を確認"]
[null,null,null,null,null,"・屋根ふき材の状況",null,null,"目視等"]
[null,"□","法23","外壁",null,"・法第22条区域の指定状況",null,null,"特定行政庁による指定状況を確認"]
[null,null,null,null,null,"・外壁材の状況",null,null,"目視等"]
[null,"□","法35の2","内装",null,"・火気使用室の有無\n・内装材",null,null,"・目視等　又は\n・材料の認定シール等を確認"]
[null,"設備関係"]
[null,null,null,null,null,"・開口部の形状等",null,null,"目視等"]
[null,null,null,null,null,"・ガス設備等の有無"]
[null,null,null,null,null,"・給気口、排気口の位置"]
[null,"□","法28②,③","換気",null,"・火気設備の出力等",null,null,"・目視等　又は\n・設備の型番から性能等を確認"]
[null,null,null,null,null,"・機械換気設備の性能等"]
[null,null,null,null,null,"・換気設備の有効換気量",null,null,"・目視等　又は\n・設備の型番から性能等を確認"]
[null,null,null,null,null,"・下水道処理区域の指定状況の確認",null,null,"地方公共団体の指定状況を確認"]
[null,null,null,null,null,"・換気、採光のための窓の有無及びそれに代わる照明\n　器具、換気設備の有無\n・漏水等の有無",null,null,"・目視等"]
[null,"□","法31","便所"]
[null,null,null,null,null,"・浄化槽の性能等",null,null,"・浄化槽の保守点検結果及び設備の\n　型番から性能等を確認"]
[null,"□","法32","電気設備",null,"・不具合の有無",null,null,"目視等"]
[null,"□","法36\n(令192の2の4)","給排水設備",null,"・配管設備の設置状況\n・漏水等の有無",null,null,"目視等"]
[null,"材料関係"]
[null,"□","法37","建築材料",null,"・基礎のコンクリート、鉄筋のJISへの適合状況",null,null,"・図書等により使用材料の仕様を確認"]
[null,"□","法28の2\n一・二","石綿",null,"・石綿の吹付けの有無",null,null,"・目視等"]
[null,"□","法28の2\n三","クロルピリホス",null,"・添加の有無(添加されている場合は、5年以上が経過\nしていること)",null,null,"・図書等により仕様を確認　又は\n・目視等"]
[null,"□",null,"ホルムアルデヒド",null,"・使用の有無(使用されている場合は、5年以上が経過\nしていること)\n・換気経路(建具のアンダーカット、ガラリ等の有無)",null,null,"・図書等による仕様を確認　又は\n・目視等"]
[null,null,null,null,null,"・換気設備の有効換気量",null,null,"・設備の型番から性能を確認"]
[null,null,null,null,null,"・居室の面積、天井高さ",null,null,"計測"]
[null,"一般構造関係"]
[null,"□","法28①","採光",null,"・照明設備の性能等",null,null,"・設備の型番から各種性能(床面において50lx以上の照度)を確認"]
[null,null,null,null,null,"・居室の面積\n・開口部の寸法、開口中心からの垂直距離\n・外壁と隣地境界線等との距離",null,null,"計測"]
[null,"□","法29","地階における居\n室",null,"・居室の面積",null,null,"計測"]
[null,null,null,null,null,"・からぼり等の有無\n・地面に接する外壁等の構造",null,null,"目視等"]
[null,"□","法36\n(令21,22)","居室の天井高さ",null,"・天井高さ",null,null,"計測"]
[null,"□",null,"居室の床高さ及\nび防湿",null,"・防湿措置(最下層の床)の状況\n・外壁の床下換気孔の状況",null,null,"目視等"]
[null,null,null,null,null,"・床の高さ",null,null,"計測"]
[null,null,null,null,null,null,null,10]

{"sheet":"sheet3 (編集)","index":24,"n_rows":31,"n_cols":7,"rows_kept":31,"cut":false,"hidden":true,"merged":[[26,1,26,3],[25,4,25,5],[13,4,13,5],[12,3,13,3],[12,2,13,2],[12,1,13,1],[14,3,15,3],[14,2,15,2],[14,1,15,1],[14,4,14,5],[16,3,17,3],[16,2,17,2],[16,1,17,1],[16,4,16,5],[19,4,19,5],[18,4,18,5],[1,6,2,6],[5,4,5,5],[6,4,6,5],[8,1,9,1],[8,3,9,3],[8,2,9,2],[9,4,9,5],[4,1,4,4],[24,4,24,5],[20,1,23,1],[20,2,23,2],[20,3,21,3],[23,4,23,5],[24,1,25,1],[24,2,25,2],[24,3,25,3],[20,4,20,5],[21,4,21,5],[22,3,23,3],[22,4,22,5],[17,4,17,5],[18,1,19,1],[18,2,19,2],[18,3,19,3],[10,1,11,1],[11,4,11,5],[10,3,11,3],[10,2,11,2],[27,1,28,1],[27,2,28,2],[27,4,28,5],[1,1,2,1],[1,2,2,2],[1,3,2,3],[1,4,2,5],[3,4,3,5],[5,1,6,1],[5,2,6,2],[5,3,6,3],[7,1,7,4],[8,4,8,5],[10,4,10,5],[12,4,12,5],[15,4,15,5]]}
[]
[null,"適用","法令","規定の内容","調査項目",null,"調査方法"]
[]
[null,"□","法36\n(令23～26)","階段","・階段及び踊場の幅員\n・階段の蹴上げ、踏面の寸法\n・手すりの設置状況、出幅の寸法\n・踊場の設置状況\n・階段に代わる傾斜路の設置状況",null,"自視等及び計測"]
[null,"用途関係(都市計画区域及び準都市計画区域内に限り適用)"]
[null,"□","法48,49","用途","・用途地域、特別用途地区の指定状況",null,"市区町村の都市計画情報を確認"]
[null,null,null,null,"・兼用用途の有無及び当該用途に供する床面積",null,"目視等及び計測"]
[null,"形態関係(都市計画区域及び準都市計画区域内に限り適用)"]
[null,"□","法47","壁面線","・壁面線の指定状況",null,"特定行政庁による指定状況を確認"]
[null,null,null,null,"・壁面線の外壁との距離",null,"計測"]
[null,"□","法52","容積率","・指定容積率",null,"市区町村の都市計画情報を確認"]
[null,null,null,null,"・建築物の延べ面積及び敷地面積\n・前面道路幅員",null,"計測"]
[null,"□","法53","建蔽率","・指定建蔽率\n・防火地域、準防火地域の指定状況",null,"市区町村の都市計画情報を確認"]
[null,null,null,null,"・建築物の建築面積及び敷地面積",null,"計測"]
[null,"□","法53の2","最低敷地面積","・敷地面積の最低限度の指定状況",null,"市区町村の都市計画情報を確認"]
[null,null,null,null,"・敷地面積",null,"計測"]
[null,"□","法54","外壁後退距離","・外壁の後退距離の限度の指定状況",null,"市区町村の都市計画情報を確認"]
[null,null,null,null,"・外壁から敷地境界線までの距離",null,"計測"]
[null,"□","法55","絶対高さ制限","・高さの限度の指定状況",null,"市区町村の都市計画情報を確認"]
[null,null,null,null,"・建築物の高さ",null,"計測"]
[null,"□","法56","道路高さ制限","・用途地域の指定状況",null,"市区町村の都市計画情報を確認"]
[null,null,null,null,"・前面道路幅員\n・前面道路との高低差\n・建築物の高さ\n・道路境界線との距離",null,"計測"]
[null,null,null,"北側高さ制限","・用途地域の指定状況\n・日影による高さ制限の対象区域の指定状況",null,"市区町村の都市計画情報及び条例の制定状況を確認"]
[null,null,null,null,"・真北の方角\n・真北方向の境界線との距離\n・北側隣地との高低差\n・建築物の高さ",null,"計測"]
[null,"□","法58","高度地区内の建\n築物","・高度地区の指定状況",null,"市区町村の都市計画情報を確認"]
[null,null,null,null,"・建築物の高さ",null,"計測"]
[null,"その他(条例により付加された制限)"]
[null,"□","法39、40、\n68の2他","地方公共団体の","地方公共団体の条例による制限の有無及び内容",null,"・条例の制定状況を確認"]
[null,null,null,"条例による制限",null,null,"・制限の内容に応じて確認方法を検討"]
[]
[null,null,null,null,null,11]

{"sheet":"sheet1","index":25,"n_rows":36,"n_cols":13,"rows_kept":36,"cut":false,"hidden":true,"merged":[[1,1,1,11],[2,1,2,11],[3,1,3,11],[4,1,4,11],[5,1,5,11],[6,1,6,11],[7,1,7,11],[8,1,8,11],[9,1,9,11],[10,1,10,11],[11,7,11,8],[13,1,13,8],[14,2,14,3],[14,4,14,5],[14,6,14,8],[15,1,17,1],[15,2,17,3],[15,4,17,5],[15,6,15,8],[15,10,17,10],[15,11,17,11],[15,12,17,12],[16,6,16,8],[17,6,17,8],[18,2,18,3],[18,4,18,5],[18,6,18,8],[19,1,19,2],[20,1,21,1],[20,2,33,3],[20,4,21,5],[20,6,20,8],[23,4,23,5],[23,6,23,8],[26,4,26,5],[26,6,26,8],[30,1,31,1],[30,4,31,5],[30,6,30,8],[33,4,33,5],[33,6,33,8],[20,9,20,11],[21,6,21,8],[21,9,21,11],[22,4,22,5],[22,6,22,8],[22,9,22,11],[23,9,23,11],[24,4,24,5],[24,6,24,8],[24,9,24,11],[25,4,25,5],[25,6,25,8],[25,9,25,11],[26,9,26,11],[27,4,27,5],[27,6,27,8],[27,9,27,11],[28,1,29,1],[28,4,29,5],[28,6,29,8],[28,9,28,11],[29,9,29,11],[33,9,33,11],[30,9,31,11],[31,6,31,8],[32,4,32,5],[32,6,32,8],[32,9,32,11]]}
[]
[null,"翻調査項目チmックリスト"]
[null,"本チェックリストは、計画建築物が2階建ての木造一戸建ての住宅(軸組工法)である場合を想定し"]
[null,"たものとしています。一般的に、2階建ての木造一戸建ての住宅の規模の建築物であれば、部位によ"]
[null,"り部材や施工方法を大きく変えることはないと考えられることから、現地で適切に適合状況を調査"]
[null,"できる箇所を選定して、隠蔽部については規定ごとに少なくとも1箇所以上(構造関係にあっては、"]
[null,"各階1箇所以上)を調査します。また、施工状況が分かる図書等があり、使用されている材料の種類"]
[null,"や寸法等が確認できる場合は、調査の一部を省略することができます。"]
[null,"それ以外の建築物である場合には、計画建築物の構造種別や用途に応じて必要な規定を適宜追加"]
[null,"するなどしてください。なお、構造関係規定については、仕様規定によらずに構造計算によって構造"]
[null,"耐力上安全であることを確かめることができる場合には、「適合」とすることができます。"]
[null,"翻",null,"法令",null,"規定の内容",null,"調査項目",null,null,"調査方法"]
[]
[null,"敷地関係(法第43条及び第44条は都市計画区域及び準都市計画区域内に限り適用)"]
[null,"口","法19",null,"敷地",null,"・敷地内の排水状況\n・敷地内の不同沈下、傾斜等の状況\n・擁壁等敷地内の安全上の措置の状況",null,null,"目視等及び言お則"]
[null,"口","法43",null,"髄",null,"・特定行政庁による道路の指定状況\n一i.1A1--111",null,null,"一一一一","特定行政庁の指定道路図を確認\n一一一\ni-.","一一\n一","一一\n一一i-一"]
[null,null,null,null,null,null,"・特定行政庁による許可・認定の有無と適合状況\nS111",null,null,"図書及び目視等\n一　ii.　一"]
[null,null,null,null,null,null,"・道路との接道長さ\n・前面道路幅員",null,null,"計測"]
[null,"口","法44",null,"道路内建築",null,"・道路、建築物、擁壁等の位置",null,null,"目視等"]
[null,"構造関係"]
[null,"口","法20",null,"基礎",null,"・立ち上がり部分の基礎の構造、材料及び寸法\n一一一一一i-一一一一一一一一\n・基礎の配筋間隔、鉄筋径等の状況",null,null,"目視等及び計測\n闇　　　　　　　　　　　　　　　　　　　　　　　　　　　　　　　　　　　AA\n・電磁誘導法又は\n・電磁波レーダL法による鉄筋探査及び\nはつり出し"]
[null,null,null,null,null,null,"・(令第38条第4項の構造計算による場合)コンクリー\nトの強度",null,null,"・コンクリート圧縮試験又は\n・シュミットハンマー試験"]
[null,"口",null,null,"屋根ふき材\n外装材等",null,"・緊結等の状況",null,null,"目視等"]
[null,"口",null,null,"木材",null,"・構造耐力上主要な部分に使用されている木材の状況",null,null,"自視等"]
[null,"[]",null,null,"土台及び基礎",null,"・土台の緊結等の状況",null,null,"圏視等"]
[null,"口",null,null,"柱の小径",null,"・欠込み等の有無\n一一一一一一一一一一一i-一一一一一一\n・部材寸法(柱の小径)",null,null,"目視等\n計測"]
[null,"口",null,null,"はり等の横架材",null,"・欠込み等の有無",null,null,"目視等"]
[null,"口",null,null,"筋かい",null,"・柱梁接合部及び筋かいの金物の有無及び金物種類、\n緊結の状況\n・欠込み等の有無\nAA　A　A　A　AA1　1AA　11　..\n・筋かいの部材寸法",null,null,"目視等\n11AA「「..11-1「一.一一一一一一.i.一\n計測"]
[null,"[]",null,null,"軸組等",null,"筋かい、耐力壁の位置\n・金物種類\n　　　　　　　　　　　　　　　　　　　　　　　　　　　　　　　　　　　　　　　　　　　　　　　　　　　　　　　　　　　　AAA　AA\n・筋かい、耐力壁の部材寸法等の状況\n一一一一一一一一一一一一一A\n壁量計算による必要壁量及び存在壁量、配置の確認\n壁配置のバランス",null,null,"目視等"]
[null,null,null,null,null,null,null,null,null,"顛視等及び計測\n　　　　　　　　　　　　　　　　　AA　AA　AAA\n壁量計算"]
[null,"口",null,null,"継手又は仕口",null,"・柱梁接合部の金物の有無及び金物種類、緊結の状況",null,null,"目視等\n一一一一一.一\n計測"]
[null,null,null,null,null,null,"「1A-1「A11AAA\n・筋かいの部材寸法"]
[null,"口",null,null,"防腐措置",null,"・腐りやすい構造である部分の下地材\n・柱、筋かい、土台の防腐・防蟻処理の状況",null,null,"目視等"]
[null,"〔]",null,null,"塀",null,"・塀の高さ、厚さ\n・控え壁、基礎の有無、塀の健金性\nAA　　　　　闇　　　　　　　　　　　　　A　A　AA　A11A　A1.　　一「1.\n・塀の配筋間隔、鉄筋径等の状況",null,null,"目視等及び計測\n一一i-一一一一i-一一一一一一\n・電磁誘導法又は"]
[]
[null,null,null,null,null,null,null,null,9]

{"sheet":"sheet2","index":26,"n_rows":37,"n_cols":10,"rows_kept":37,"cut":false,"hidden":true,"merged":[[1,1,1,2],[1,6,1,7],[2,2,3,2],[2,3,2,4],[2,5,2,7],[2,8,2,9],[3,3,3,4],[3,5,3,7],[3,8,3,9],[4,1,4,2],[5,3,5,4],[5,5,5,7],[5,8,5,9],[6,3,6,4],[6,5,6,7],[6,8,6,9],[7,1,8,1],[7,2,8,2],[7,3,8,4],[7,5,7,7],[7,8,7,9],[8,5,8,7],[8,8,8,9],[9,3,9,4],[9,5,9,7],[9,8,9,9],[10,3,10,4],[10,5,10,7],[10,8,10,9],[11,1,11,2],[12,3,12,4],[12,5,12,7],[12,8,12,9],[13,3,13,4],[13,5,13,7],[13,8,13,9],[14,3,14,4],[14,5,14,7],[14,8,14,9],[15,3,15,4],[15,5,15,7],[15,8,15,9],[16,3,16,4],[16,5,16,7],[16,8,16,9],[17,3,17,4],[17,5,17,7],[17,9,17,9],[18,3,18,4],[18,5,18,7],[18,8,18,9],[19,3,19,4],[19,5,19,7],[19,8,19,9],[20,3,20,4],[20,5,20,7],[20,8,20,9],[21,3,21,4],[21,5,21,7],[21,9,21,9],[22,3,22,4],[22,5,22,7],[23,3,23,4],[23,5,23,7],[24,1,24,2],[25,3,25,4],[25,5,25,7],[26,3,26,4],[26,5,26,7],[27,2,29,2],[27,3,27,4],[27,5,27,7],[28,1,29,1],[28,3,29,4],[28,5,28,7],[28,8,29,8],[29,5,29,7],[30,1,30,2],[31,3,31,4],[31,5,31,7],[32,3,32,4],[32,5,32,7],[33,2,34,2],[33,3,33,4],[33,5,33,7],[34,3,34,4],[34,5,34,7]]}
[]
[null,"適用法令",null,null,"規定の内容",null,"調査項目",null,null,"調査方法"]
[null,null,null,null,null,null,null,null,"・電磁波レーダー法による鉄筋探査及び\nはつり出し"]
[null,"口",null,"建築設備の構造\n強度",null,"・給湯設備の満水時の質量\n・給湯設備の形状\n・給湯設備の緊結状況",null,null,"・設備の型番から仕様を確認\n・目視等"]
[null,"防火関係"]
[null,"口","法61","防火地域準防火\n地域内の建築物",null,"・防火地域、準防火地域の指定状況\n　　　　　　　　　　　　A　\"AAA　A　AA　AA\n・建築物の規模に応じた耐火建築物、準耐火建築物等\nの種別及び構造材の状況\n・延焼のおそれのある部分の防火設備の位置、形状等",null,null,"市区町村の都市計画情報を確認\nAAA「1AA11-\n・目視等又は\n・設備の認定シール等を確認"]
[null,"口","法62","屋根",null,"・防火地域、準防火地域の指定状況\n一i-一一一一一一一一一一一一一一一\n・屋根材の状況",null,null,"市区町村の都市計画情報を確認\n一一一一一\n目視等"]
[null,"[]","法22","屋根",null,"・法第22条区域の指定状況\n　　　　　　　　　　　　　　　　　　　　　　　　　　　　　　　　AA1",null,null,"特定行政庁による指定状況を確認\n..11-1-一"]
[null,null,null,null,null,"・屋根δ、き材の状況",null,null,"目視等"]
[null,"〔]","法23","外壁",null,"・法第22条区域の指定状況\nA\n・外壁材の状況",null,null,"特定行政庁による指定状況を確認\n一A「\n目視等"]
[null,"[コ","法35の2","内装",null,"・火気使用室の有無\n・内装材",null,null,"・目視等又は\n・材料の認定シール等を確認"]
[null,"設備関係"]
[null,null,null,null,null,"・開口部の形状等"]
[null,null,null,null,null,"・ガス設備等の有無",null,null,"目視等"]
[null,null,null,null,null,"・給気口、排気口の位置"]
[null,"口","法28②,③","換気",null,"一一一一一一i-一一\n・火気設備の出力等",null,null,"一一\n・目視等又は"]
[null,null,null,null,null,"機械換気設備の性能等",null,null,"・設備の型番から性能等を確認"]
[null,null,null,null,null,"1-1111A1A1111AA1111AA1111.1A「1.1111\n・換気設備の有効換気量",null,null,".1AA.\n・圏視等又は\n・設備の型番から性能等を確認"]
[null,null,null,null,null,"・下水道処理区域の指定状況の確認\n.1111111A1111AA11.1AA「11.AA1-1",null,null,"地方公共団体の指定状況を確認\n一一一.1i-一一"]
[null,null,null,null,null,"・換気、採光のための窓の有無及びそれに代わる照明"]
[null,"口","法31","便所",null,"器具、換気設備の有無\n・漏水等の有無",null,null,"・目視等"]
[null,null,null,null,null,"一一一一一一一一一一一.1-.i.i-一一一一一一一一\n・浄化槽の性能等",null,null,"一一一一一一一一一一\n・浄化槽の保守点検結果及び設備の\n型番から性能等を確認"]
[null,"〔コ","法32","電気設備",null,"・不具合の有無",null,null,"目視等"]
[null,"口","法36\n〔令129の2の4)","給排水設備",null,"・配管設備の設置状況\n・漏水等の有無",null,null,"目視等"]
[null,"材料関係"]
[null,"口","法37","建築材料",null,"・基礎のコンクリート、鉄筋の丑Sへの適合状況",null,null,"・図書等により使用材料の仕様を確認"]
[null,"口","法28の2\n-・二","石綿",null,"・石綿の吹付けの有無",null,null,"・圏視等"]
[null,"口","法28の2\n三","クロルピリホス",null,"・添加の有無(添加されている場合は、5年以上が経過\nしていること)",null,null,"・図書等により仕様を確認又は\n・目視等"]
[null,"口",null,"ホルムアルデヒド",null,"・使用の有無(使用されている場合は、5年以上が経過\nしていること)\n・換気経路(建具のアンダーカット、ガラリ等の有無)\nA　AA　AAA　A1　AA1\n・換気設備の有効換気量\n11...1A",null,null,"・図書等による仕様を確認又は\n・目視等\n11111A1AA「11111「11..1.一\n・設備の型番から性能等を確認\n一.-i-一一一一一一\n計測"]
[null,null,null,null,null,"・居室の面積、天井高さ"]
[null,"一般構造関係"]
[null,"口","法28①","採光",null,"・照明設備の性能等\n闇　　　　　　　　　　　　　　　　　　A　AAA　A\n・居室の面積\n・開口部の寸法、開口中心からの垂直距離\n・外壁と隣地境界線等との距離",null,null,"・設備の型番から各種性能(床面にお\nいて5αx以上の照度)を確認\n11AA1111A111\n計測"]
[null,"口","法29","地階における居\n室",null,"・居室の面積\n一一一一一一一一一一i-一一一一一一一一一一一一\n・からぼり等の有無\n・地面に接する外壁等の構造",null,null,"計測\n一一一一一\n目視等"]
[null,"口","法36\n(令21,22)","居室の天井高さ",null,"・天井高さ",null,null,"計測"]
[null,"口",null,"居室の床高さ及\nび防湿",null,"・防湿措置(最下層の床の材料)の状況\n・外壁の床下換気孔の状況\n一一一一一一一一一闇\"\n・床の高さ",null,null,"目視等\n一\n計測"]
[]
[null,null,null,null,null,null,null,10]

{"sheet":"sheet3","index":27,"n_rows":25,"n_cols":7,"rows_kept":25,"cut":false,"hidden":true,"merged":[[1,1,2,1],[1,2,2,2],[1,3,2,3],[1,4,2,5],[1,6,1,6],[3,4,3,5],[4,1,4,4],[5,1,6,1],[5,2,6,2],[5,3,6,3],[5,4,6,5],[7,1,7,4],[8,4,8,5],[9,4,9,5],[10,4,10,5],[11,4,11,5],[12,4,12,5],[13,1,14,1],[13,2,14,2],[13,3,14,3],[13,4,14,5],[18,6,19,6],[15,1,17,1],[15,2,17,2],[15,3,16,3],[15,4,16,5],[15,6,16,6],[17,4,17,5],[20,1,20,3],[22,4,22,5],[18,1,19,1],[18,2,19,2],[18,3,19,3],[18,4,19,5]]}
[]
[null,"観","法令","規定の内容","調査項目",null,"調査方法"]
[null,null,null,null,null,null,"介"]
[null,"口","法36\n(令23～26)","階段","・階段及び踊場の幅員\n・階段の蹴上げ、踏面の寸法\n・手すりの設置状況、出幅の寸法\n・踊場の設置状況\n・階段に代わる傾斜路の設置状況",null,"自視等及び計測"]
[null,"用途関係(都市計画区域及び準都市計画区域内に限り適用)"]
[null,"[]","法48,49","用途","・用途地域、特別用途地区の指定状況\n　　　　　　　　　　　　　　　　　　　　　　　　　A　「AA1\n・兼用用途の有無及び当該用途に供する床面積",null,"市区町村の都市計画情報を確認"]
[null,null,null,null,null,null,"目視等及び計測"]
[null,"形態関係(都市計画区域及び準都市計画区域内に限り適用)"]
[null,"[]","法47","壁面線","・壁面線の指定状況\n一一一一i-一一一一一\n壁面線と外壁との距離",null,"特定行政庁による指定状況を確認\n　　　　　　　　　　　　　　　　　　　　　　　　　　　　　　　　　　　　　　　A　AAA　1.\n計測"]
[null,"E]","法52","容積率","・指定容積率\niiis11-一一一.一一一一一一1-一一一一一\n・建築物の延べ面積及び敷地面積\n・前面道路幅員",null,"市区町村の都市計画1青報を確認\n\"　AA　lli　一\n計測"]
[null,"[]","法53","建蔽率","指定建蔽率\n・防火地域、準防火地域の指定状況\nAA1AA「1.\n・建築物の建築面積及び敷地面積",null,"市区町村の都市計画情報を確認\n11.一一11-.11.一\n計測"]
[null,"口","法53の2","最低敷地面積","・敷地面積の最低限度の指定状況\nA\n・敷地面積",null,"市区町村の都市計画情報を確認\n一一一i-一一闇\n計測"]
[null,"〔]","法54","外壁後退距離","・外壁の後退距離の限度の指定状況\n1.11-一一.一\n・外壁から敷地境界線までの距離",null,"市区町村の都市計画庸報を確認\n一　　　　　　　　　　　　　　　　　　　　　　　　　　　　　　　　　　　　　　　　　　　AA.\n計測"]
[null,"口","法55","絶対高亡制限","・高さの限度の指定状況\n11「\n健築物の高さ",null,"市区町村の都市計画情報を確認\n一一一"]
[null,null,null,null,null,null,"計測"]
[null,"口","法56","道路高さ制限","湖途地域の指定状況\nAA1A1AAA11A1.1\n・前面道路幅員\n・前面道路との高低差\n・建築物の高さ\n・道路境界線との距離",null,"市区町村の都市計画情報を確認\n一一一幽一一一一一\n計測"]
[]
[null,null,null,"北側高さ制限","・用途地域の指定状況\n・日影による高さ制限の対象区域の指定状況\n一一一一一一一一一一一一一一一一A\n・真北の方角\n・真北方向の境界線との距離\n・北側隣地との高低差\n・建築物の高さ",null,"市区町村の都市計画情報及び条例の\n制定状況を確認\nAAA11.111-.11.一.\n計測"]
[null,"口","法58","高度地区内の建\n築物","・高度地区の指定状況\n闇　　　　　　　　　　A　A　AAA　AA　A11\n健築物の高さ",null,"市区町村の都市計画惰報を確認\n一一一一一一一\n計測"]
[]
[null,"その他(条例により付加された制限)"]
[null,null,"法39,40,","地方公共団体の",null,null,"・条例の制定状況を確認"]
[null,null,"68の2他","条例による制限","地方公共団体の条例による制限の有無及び内容",null,"・制限の内容に応じて確認方法を検討"]
[]
[null,null,null,null,null,11]